ATTO ExpressSAS RAID Controller Windows ReadMe Package Contents Supported Adapters Installation Instructions Windows 2000 & XP Windows Server 2003 Windows Vista & Server 2008 Creating ExpressSAS Installation Media Registry Settings Driver Events Contact Info Package Contents
attomtln.cat | ATTO phantom device driver catalog file
attomtln.inf | ATTO phantom device driver installation file
esasraid | Signature file
esasraid.cat | Windows ExpressSAS driver catalog file
esasraid.inf | Windows ExpressSAS driver installation file
esasraid.sys | Windows ExpressSAS driver
ReadMe.htm | Release notes
Setup.exe | Driver installer
txtsetup.oem | Windows text-based setup installation file
Supported Adapters ATTO ExpressSAS R348 ATTO ExpressSAS R380 ATTO ExpressSAS R30F Installation Instructions Windows 2000 & XP Windows Server 2003 Windows Vista & Server 2008 Creating ExpressSAS Installation Media Note: If you already have one or more ExpressSAS adapters installed and you are installing additional adapters, you do NOT need to perform any of these procedures unless you are updating a previously installed driver. Windows 2000 & XP Installation Upgrading your ExpressSAS Windows driver Adding an ExpressSAS adapter to an existing Windows installation Installing a fresh copy of Windows onto a disk attached to the ExpressSAS adapter Upgrading your ExpressSAS Windows driver To install from the ExpressSAS Installation CD: Log on to Windows as the system administrator. Insert the ExpressSAS Installation CD into a CD or DVD drive and the CD will automatically start. If the CD does not start, navigate to the root of the CD and run 'autorun.bat'. Select "Windows Drivers" from the items on the left side of the screen. Select the appropriate CPU based operating system from operating system choices. Select "Install Windows Driver" to launch the driver installer. Click 'Install' and follow the on-screen instructions to complete the driver installation. To install from the ATTO Technology website: Log on to Windows as the system administrator. Go to the Downloads section of www.attotech.com and locate the driver download for your adapter and operating system. Click on the link to download the file. Internet Explorer users may select 'Run' to automatically run the downloaded self-extracting executable. Otherwise, select a download destination and run the self-extracting executable when the download is complete. Click 'Unzip' to extract the driver files and launch the driver installer. Click 'Install' and follow the on-screen instructions to complete the driver installation. To install from a directory containing the ExpressSAS driver: Log on to Windows as the system administrator. Navigate to the directory containing the ExpressSAS driver and run Setup.exe. Click 'Install' and follow the on-screen instructions to complete the driver installation. Adding an ExpressSAS adapter to an existing Windows installation Note: It is recommended that you complete this installation procedure before attaching any devices to the adapter. Perform the installation procedure in (A) to pre-install the ExpressSAS driver. Shutdown Windows when Setup prompts you to do so. Install your ExpressSAS adapter into an available PCI expansion slot. Restart Windows. Windows should detect your ExpressSAS adapter and the Found New Hardware Wizard should appear. Proceed through the wizard with the default settings for each adapter channel. During the installation, you may be prompted to insert the ExpressSAS installation media. Make sure that the driver you used in procedure (A) is present and click 'OK' to continue installation. When adapter installation is complete, the Found New Hardware Wizard will appear for an "ATTO Phantom Device" for each channel. Proceed through the wizard with the default settings to complete the installation. Shutdown the system and setup the final adapter configuration. If the ExpressSAS adapter is replacing another adapter in the system, disconnect the cables from the adapter and remove the adapter from the system. Optionally, you can move the ExpressSAS adapter to the PCI slot that the previous adapter occupied if this slot is more suitable for the ExpressSAS adapter. Attach the appropriate cables to the ExpressSAS adapter. Close the computer chassis, turn on the power and restart Windows. Note: If you moved the adapter to a different PCI slot, the Found New Hardware Wizard will appear. Proceed through the wizard with the default settings for each adapter channel to complete the installation. Installing a fresh copy of Windows onto a disk attached to the ExpressSAS adapter Note: A floppy disk with the ExpressSAS driver software is required to complete this procedure. See Creating ExpressSAS Installation Media. Start Windows text mode setup as per the instructions provided with Windows. Press F6 when the first blue window appears called "Windows Setup". The setup program will display a prompt in the status window on the bottom left of the monitor. Setup will continue to load files after you press F6. A new window will appear that gives instructions to specify additional mass storage devices. Press 'S' indiciating that you wish to install a storage device. Insert the ExpressSAS installation floppy disk in drive A: and press Enter. You should then be presented with a screen from which you would normally select a driver, but only a list of ExpressSAS adapters should appear. Select your adapter and Press Enter. Windows Setup will load the files from the floppy and then display screen described in step 2. The 'ATTO ExpressSAS' device should now be listed as detected. Repeat steps 2 - 4 for any other vendor-supplied driver installation disks. After all other drivers have been processed, press Enter and proceed with the rest of the Windows installation procedure. Note: When Windows begins copying files to your hard disk, you will again be prompted to insert the ExpressSAS installation floppy disk (and any other vendor-supplied disks you used during custom installation). This is normal. The first time you inserted the disks, Windows only loaded the drivers into memory; the second time you insert the disk(s), Windows is copying the driver to your hard disk. Windows Server 2003 Installation Upgrading your ExpressSAS Windows driver Adding an ExpressSAS adapter to an existing Windows installation Installing a fresh copy of Windows onto a disk attached to the ExpressSAS adapter Upgrading your ExpressSAS Windows driver Note: It is strongly recommended that you update to Windows Server 2003 SP1 or later before installing the ExpressSAS driver. To install from the ExpressSAS Installation CD: Log on to Windows as the system administrator. Insert the ExpressSAS Installation CD into a CD or DVD drive and the CD will automatically start. If the CD does not start, navigate to the root of the CD and run 'autorun.bat'. Select "Windows Drivers" from the items on the left side of the screen. Select the appropriate CPU based operating system from operating system choices. Select "Install Windows Driver" to launch the driver installer. Click 'Install' and follow the on-screen instructions to complete the driver installation. To install from the ATTO Technology website: Log on to Windows as the system administrator. Go to the Downloads section of www.attotech.com and locate the driver download for your adapter and operating system. Click on the link to download the file. Internet Explorer users may select 'Run' to automatically run the downloaded self-extracting executable. Otherwise, select a download destination and run the self-extracting executable when the download is complete. Click 'Unzip' to extract the driver files and launch the driver installer. Click 'Install' and follow the on-screen instructions to complete the driver installation. To install from a directory containing the ExpressSAS driver: Log on to Windows as the system administrator. Navigate to the directory containing the ExpressSAS driver and run Setup.exe. Click 'Install' and follow the on-screen instructions to complete the driver installation. Adding an ExpressSAS adapter to an existing Windows installation Note: It is recommended that you complete this installation procedure before attaching any devices to the adapter. Perform the installation procedure in (A) to pre-install the ExpressSAS driver. Shutdown Windows when Setup prompts you to do so. Install your ExpressSAS adapter into an available PCI expansion slot. Restart Windows. Windows should detect your ExpressSAS adapter and the Found New Hardware Wizard should appear. Proceed through the wizard with the default settings for each adapter channel. During the installation, you will be prompted to insert the ExpressSAS Installation media. Make sure that the driver you used in procedure (A) is present and click 'OK' to continue installation. Shutdown the system and setup the final adapter configuration. If the ExpressSAS adapter is replacing another adapter in the system, disconnect the cables from the adapter and remove the adapter from the system. Optionally, you can move the ExpressSAS adapter to the PCI slot that the previous adapter occupied if this slot is more suitable for the ExpressSAS adapter. Attach the appropriate cables to the ExpressSAS adapter. Close the computer chassis, turn on the power and restart Windows. Note: If you moved the adapter to a different PCI slot, the Found New Hardware Wizard will appear. Proceed through the wizard with the default settings for each adapter channel to complete the installation. Installing a fresh copy of Windows onto a disk attached to the ExpressSAS adapter Note: A floppy disk with the ExpressSAS driver software is required to complete this procedure. See Creating ExpressSAS Installation Media. Start Windows text mode setup as per the instructions provided with Windows. Press F6 when the first blue window appears called "Windows Setup". The setup program will display a prompt in the status window on the bottom left of the monitor. Setup will continue to load files after you press F6. A new window will appear that gives instructions to specify additional mass storage devices. Press 'S' indiciating that you wish to install a storage device. Insert the ExpressSAS installation floppy disk in drive A: and press Enter. You should then be presented with a screen from which you would normally select a driver, but only a list of ExpressSAS adapters should appear. Select your adapter and Press Enter. Windows Setup will load the files from the floppy and then display screen described in step 2. The 'ATTO ExpressSAS' device should now be listed as detected. Repeat steps 2 - 4 for any other vendor-supplied driver installation disks. After all other drivers have been processed, press Enter and proceed with the rest of the Windows installation procedure. Note: When Windows begins copying files to your hard disk, you will again be prompted to insert the ExpressSAS installation floppy disk (and any other vendor-supplied disks you used during custom installation). This is normal. The first time you inserted the disks, Windows only loaded the drivers into memory; the second time you insert the disk(s), Windows is copying the driver to your hard disk. It is strongly recommended that you update to Windows Server 2003 SP1 or later when installation is complete. Windows Vista & Server 2008 Installation Upgrading your ExpressSAS Windows driver Adding an ExpressSAS adapter to an existing Windows installation Installing a fresh copy of Windows onto a disk attached to the ExpressSAS adapter Upgrading your ExpressSAS Windows driver To install from the ExpressSAS Installation CD: Log on to Windows as the system administrator. Insert the ExpressSAS Installation CD into a CD or DVD drive and the CD will automatically start. If the CD does not start, navigate to the root of the CD and run 'autorun.bat'. Select "Windows Drivers" from the items on the left side of the screen. Select the appropriate CPU based operating system from operating system choices. Select "Install Windows Driver" to launch the driver installer. If you have User Account Control enabled, you will be prompted to grant the installer permission to continue. If you do not have administrator privileges, you will also be prompted for an administrator username and password. Click the 'Continue' button. Click 'Install' and follow the on-screen instructions to complete the driver installation. To install from the ATTO Technology website: Log on to Windows as the system administrator. Go to the Downloads section of www.attotech.com and locate the driver download for your adapter and operating system. Click on the link to download the file. Internet Explorer users may select 'Run' to automatically run the downloaded self-extracting executable. Otherwise, select a download destination and run the self-extracting executable when the download is complete. If you have User Account Control enabled, you will be prompted to grant the installer permission to continue. If you do not have administrator privileges, you will also be prompted for an administrator username and password. Click the 'Continue' button. Click 'Unzip' to extract the driver files and launch the driver installer. Click 'Install' and follow the on-screen instructions to complete the driver installation. To install from a directory containing the ExpressSAS driver: Log on to Windows as the system administrator. Navigate to the directory containing the ExpressSAS driver and run Setup.exe. If you have User Account Control enabled, you will be prompted to grant the installer permission to continue. If you do not have administrator privileges, you will also be prompted for an administrator username and password. Click the 'Continue' button. Click 'Install' and follow the on-screen instructions to complete the driver installation. Adding an ExpressSAS adapter to an existing Windows installation Note: It is recommended that you complete this installation procedure before attaching any devices to the adapter. Perform the installation procedure in (A) to pre-install the ExpressSAS driver. Shutdown Windows when Setup prompts you to do so. Install your ExpressSAS adapter into an available PCI expansion slot. Restart Windows. Windows should detect your ExpressSAS adapter and install the driver automatically. Shutdown the system and setup the final adapter configuration. If the ExpressSAS adapter is replacing another adapter in the system, disconnect the cables from the adapter and remove the adapter from the system. Optionally, you can move the ExpressSAS adapter to the PCI slot that the previous adapter occupied if this slot is more suitable for the ExpressSAS adapter. Attach the appropriate cables to the ExpressSAS adapter. Close the computer chassis, turn on the power and restart Windows. Installing a fresh copy of Windows onto a disk attached to the ExpressSAS adapter Note: Media such as the ExpressSAS Installation CD or a USB flash drive with the ExpressSAS driver software is required to complete this procedure. See Creating ExpressSAS Installation Media. Start Windows setup per the instructions provided with Windows. Select a custom installation and proceed to the 'Where do you want to install Windows?' window. Click 'Load Driver'. Insert media containing the ExpressSAS driver package and click 'OK'. Windows Setup will search for drivers matching devices in your system. If the ExpressSAS adapter is not listed in the 'Select the driver to be installed.' list, click 'Browse' and locate the driver. Select the ExpressSAS adapter from the list and click 'Next' to install the driver. You will now be back at the 'Where do you want to install Windows?' window and your devices should be listed. You may remove the ExpressSAS installation media. Configure and select a partition for installing Windows. Click 'Next'. Finish Windows installation per the instructions provided with Windows. Creating ExpressSAS Installation Media Use these procedures to transfer the ExpressSAS driver files to alternate media such as a hard drive, floppy disk, or USB flash drive for the installation procedures above. To create installation media from the ExpressSAS Installation CD: Insert the ExpressSAS Installation CD into a CD or DVD drive and the CD will automatically start. If the CD does not start, navigate to the root of the CD and run 'autorun.bat'. Select "Windows Drivers" from the items on the left side of the screen. Select the appropriate CPU based operating system from operating system choices. Select "Create Driver Installation Media" for the desired operating system. Follow the instructions for creating the installation media. To create installation media from an ExpressSAS driver download from the ATTO Technology website: Go to the Downloads section of www.attotech.com and locate the driver download for your adapter and operating system. Click on the link to download the file. Internet Explorer users may select 'Run' to automatically run the downloaded self-extracting executable. Otherwise, select a download destination and run the self-extracting executable when the download is complete. Uncheck 'When done unzipping open .\Setup.exe'. Select a different destination folder if desired and click 'Unzip' to extract the driver files. The expanded software package will contain a Scsiport driver in the base directory and a Storport driver in the Storport subdirectory. Use Scsiport for Windows 2000 and XP and use Storport for all other versions of Windows. Navigate to the folder with the desired ExpressSAS driver. Run 'makedisk.exe' and follow the instructions for creating the installation media. Registry Settings Note: Modifying your registry incorrectly may result in making your machine unbootable. Please use care in editing the registry. All registry settings are DWORD values. The following settings can be found in the registry under HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\esasraid\Parameters\Device. Settings: DisableBusChangeNotification A non-zero value causes the driver to not notify Windows of bus changes. We have found that some versions of Windows 2000 do not handle these notifications well and there may be some other circumstances where the user may not want the notifications. The default value is 0 (bus change notification enabled). EventLogMask Controls the type of events that the ExpressSAS driver writes to the system event log. Each event type is given a unique value. The sum of the values for the events you would like to see is placed in this parameter. The default value of this variable is 1, logging only fatal initialization errors. See the Driver Events section for a description of the event types. MaxXferSize Maximum data transfer size. The value, to be valid, must be at least 68KB. If this value is not present or not valid, it is assumed to be 8MB. Driver Events The reporting of driver events is controlled by the EventLogMask registry setting. EventLogMask is the sum of the event type values for the events you would like to see.
Event Type | Value (hexadecimal) | Description
Fatal | 0x00000001 | Fatal errors, always reported
SCSI | 0x00000004 | SCSI command errors
Protocol | 0x00000008 | SAS protocol errors
Login | 0x00000010 | Device login/logout events
Resource | 0x00000040 | Resource usage failures
Info | 0x00000080 | Informational messages
Underflow | 0x00000800 | Data underflow errors
In general, only errors that are output for event type 'Fatal' are significant; all others are mostly for informational or diagnostic purposes. When turning on event logging, be aware that certain events reported as errors are expected. For example, a SCSI Check Condition error will be reported for the first command sent to a device after power on or a reset condition. Also, certain data underrun errors are expected by the software and are normal. All events report the adapter number on which the event occurred. The adapter number is simply the order in which Windows initialized the adapter channels and has no relevance to what slot the adapter is in or which channel of the adapter is being reported. Contact Info You may receive customer service, sales information, and technical support by phone Monday through Friday, Eastern Standard Time 8:00 am to 8:00 pm, or by fax and web site 24 hours a day. ATTO Technology, Inc. 155 CrossPoint Parkway Amherst, New York 14068 Phone: (716) 691-1999 Fax: (716) 691-9353 www.attotech.com ATTO Technology can also be reached via e-mail at the following addresses: Sales Support: sls@attotech.com Technical Support: techsupp@attotech.com