March 03, 2020
Aquantia Windows driver release ver 2.1.20 Release notes
----------------------------------------------------------
Supported OSes: 	Windows 7, 8, 8.1, 10, Server 2012/2016/2019
Supported devices: 	AQC100, AQC107/108, AQC111/112
			AQC100S, AQC107S


Change log:
v2.1.021.0
---------------
Date 05.03.2020

- Fixed checksums which were reported to OS for packets with non-zero padding

v2.1.020.0
---------------
Date 05.02.2020

- Edimax HWID was added
- Disabled EEE for 1Gbit/s link speed 
- Enabled EEE for specific HWID 
- Added HWIDs for HP Flatiron 
- Fixed issue with ring overflow if device receives a lot of corrupted Ethernet frames
- Added SNR data for cable diagnostic
- Improved performance on Hyper-V guest


Change log:
v2.1.019.0
---------------
Date 25.10.2019

- Fixed issue with ring overflow if device receives a lot of corrupted Ethernet frames
- Added SNR data for cable diagnostic
- Improved performance on Hyper-V guest
- Added Lenovo IDs

v2.1.018.0
---------------
Date 05.06.2019

- Fixed warning message about loss of the link on every system restart
- Fixed RSC traffic stuck under heavy load
- Fixed retransmission of packets with 0xFFFF checksum
- Changed RSS queues numbers

v2.1.017.0
---------------
Date 19.02.2019

- Fixed issue when packets markes as invalid if packets have non-zero padding
- Thermal shutdown management added
- Changed default value for RSC settings on Gigabyte HWIDs

v2.1.016.0
---------------
Date 21.12.2018

- Fix spontaneous disconnects and data path stuck on AQC111

v2.1.012.0
---------------
Date 08.11.2018

- Several driver strings were changed
- Link Speed setting was changed for ASUS XG-C100F
- Passed WHQL testing for Windows 10RS5

v2.1.010.0
---------------
Date 29.09.2018

- Service name changed to match the driver name.
- Fix for receive path stuck under heavy load.
- Fix for statistics not reported correctly via WMI (MSFT_NetAdapterStatisticsSettingData class).
- Fix for flow control settings not configured correctly in some cases.


v2.1.009.0
---------------
Date 03.08.2018

- PHY temperature reported via WMI is always zero.

v2.1.008.0
---------------
Date 04.07.2018

- Changes in error handling for resource allocation. Previous version could cause BSoD

v2.1.007.0
---------------
Date 03.07.2018

- Added Tx stuck Firmware interrupt handler that triggers Tx path reset sequence in both H/W and S/W.
- Strict speed policy - only chosen speed is advertised.
- Perform NIC reset when PHY global fault is detected on AQC100 (Applicable to Aquantia SFP modules). 
- Take control over eFUSE before reading (important fix for secure chips because driiver reads secure hash from eFuse).
- New Tx data path w/SGDMA.



v2.1.006.0
---------------
Date 26.05.2018

- Reallocate stale NBLs instead of using work item after suspend resume
- Major code refactoring

